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See Standard Specifications for Degree of Compaction Requirements.  Notify Project Manager and indicate action taken on all tests below the contract requirements.
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