000-Notes to designer: (DELETE FROM CONTRACT)
1. Foundation Drilling, Item SPV.0090.xx
A  Description
This special provision describes providing work consisting of drilling or otherwise excavating holes for the subsequent installation of soldier piles and construction of concrete masonry soldier pile footings. Perform work according to pertinent parts of the standard specifications, the plans, and these special provisions.
B  Materials (Vacant)
C  Construction
C.1  General
The contractor is responsible for drilling or excavating and maintaining a stable open hole for subsequent installation of soldier piles and construction of concrete masonry soldier pile footings. Partial or full depth temporary casing, drilling fluid or a combination thereof, may be required to maintain the stability of the excavated drill hole prior to placement of the soldier pile in the hole and filling the hole with concrete. Use a dry method or wet method to maintain a stable open hole.
C.2  Installation Plan Submittal
[bookmark: _Hlk231301327]Determine the proper means, methods, and procedure for accomplishing the work as specified herein and on the plans. Submit the proposed method for foundation drilling before beginning construction. If drilling fluid is proposed to be used for excavation stabilization, the submitted installation plan must include all details related to use of drilling fluid including:
1. Type: Include drilling fluid manufacture literature and mixing instructions.
2. Equipment: Storage /mixing tanks, containment vessels, pumps, mixers, hoses, valves.
3. Operations: Drilling fluid mixing, pumping, containment, and recovery procedures.
4. Quality Control: Drilling fluid quality control procedures and testing during construction. 
C.3  Excavation
Drill or otherwise excavate holes to the diameter and depth as shown on the plans. If necessary, use temporary casing, drilling fluid or alternative methods during drilling methods to maintain a stable open hole. Do not leave excavated, uncased holes open overnight prior to filling with concrete. If bentonite or equivalent drilling fluid is used to maintain an open hole, prevent spillage of the drilling fluid onto adjacent roadways or into adjacent waterways. Locate the soldier pile holes within the following tolerances:
	Horizontal Location
	3 inches

	Vertical Location
	1 inch

	Vertical Alignment
	1/8 inch per foot

	Hole Diameter
	-0 inch; +2 inch


		Provide equipment for checking the dimensions and alignment of each shaft. Remove loose material from the bottom of the shaft. For holes drilled or excavated with the dry method, no more than 3 inches of standing water is permitted in the bottom of the drilled hole prior to beginning solider pile installation and immediately prior to placing concrete masonry in the hole around the solider pile.
D  Measurement
The department will measure Foundation Drilling by the linear foot, acceptably completed.
E  Payment
The department will pay for measured quantities at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0090.xx	Foundation Drilling	LF
Payment is full compensation for drilling foundations; for drilling or otherwise excavating holes, for coring rock, for furnishing temporary casings, drilling fluid or alternative hole stabilization methods, and disposal of all excavated material and drilling fluid.
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