000-Notes to designer: (DELETE FROM CONTRACT)
1. Timber Lagging, Item SPV.0110.xx
A  Description
This special provision describes furnishing, delivering, and installing all temporary timber lagging for soldier pile and lagging walls. Perform work according to pertinent parts of the standard specifications, the plans, and these special provisions.
B  Materials
Furnish materials that conform to lumber as specified in standard spec 507 except that preservative treatments according to standard spec 507.2.2.6 are not required and untreated lumber may be used. Use Douglas fir-larch or Southern pine construction grade rough-cut lumber with a minimum thickness of 3-inches. Where necessary provide certification that the timber conforms to the grade, species, and other specified requirements.
Alternate lagging materials, with properties equal to or better than above requirements, or provisionary lagging with a design signed and sealed by a professional engineer currently registered in the state of Wisconsin may be submitted to the engineer for approval.  No additional compensation will be paid to contractor for use of any approved alternate materials or systems.
C  Construction
Place timber lagging from the top-down in sufficiently small lifts immediately after excavation to prevent erosion of materials into excavation. Before placing lagging, smooth the soil face to create a contact surface for the lagging. Backfill and compact large voids behind the lagging. Unless the plans show otherwise, maintain a 3/4-inch gap between each vertically adjacent board for drainage between adjacent lagging sections. Never place lagging in tight contact to adjacent lagging.
D  Measurement
The department will measure Timber Lagging by the thousand feet board measure (MBM), acceptably completed. The department will compute the measured quantity from the theoretical pay limits the contract plans show. The department will make no allowance for wall area constructed above or below the theoretical pay limits. All work beyond the theoretical pay limits is incidental to the cost of work. The department will make no allowance for as-built quantities.
E  Payment
The department will pay for measured quantities at the contract unit price under the following bid item:
ITEM NUMBER	DESCRIPTION	UNIT
SPV.0110.XX	Timber Lagging	MBM
Payment is full compensation for providing, framing, and placing; and for materials and hardware required for erecting the timber.
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