**CONSTRUCTION EROSION AND SEDIMENT INSPECTION**

Wisconsin Department of Transportation

DT1072 2/2020

**1. Project Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Project Engineer** |  | **Project ID** |  |
| **Field Office Phone** |  | **Roadway** |  |
| **Prime Contractor** |  | **Description** |  |
| **EC Sub-Contractor** |  | **County** |  |

**2. Inspection Information**

|  |  |  |
| --- | --- | --- |
| **Inspector Name:**  | **Inspection Date:**  | **Weather:**  |
| **Reason for inspection:** **[ ]  Weekly** **[ ]  ≥ 0.5 in. rain in 24 hours** **[ ]  Stage** **[ ]  Other:**  |
| **Estimated percent of project open and not landscaped:**  |
| **Was the Prime Contractor present for inspection?**  |
| **Were all project BMPs inspected, including BMPs on Contractor Disturbed Areas (equipment staging, material storage, select sites, etc.)?** (if no, explain) |
| **General comments: (i.e. description of current phase of construction, schedule changes that may increase sediment discharge, environmentally sensitive areas inspected for evidence of sediment, topics for construction update meetings, etc.)**  |

**3. Project and Select Site, Best Management Practices (BMPs)**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Modifications Required:** | YES | NO | N/A | **Modifications Required:** | YES | NO | N/A |
| Silt Fence | [ ]  | [ ]  | [ ]  | Mulch | [ ]  | [ ]  | [ ]  |
| Ditch Checks | [ ]  | [ ]  | [ ]  | Erosion Mat | [ ]  | [ ]  | [ ]  |
| Silt Screen | [ ]  | [ ]  | [ ]  | Temporary Seeding | [ ]  | [ ]  | [ ]  |
| Riprap | [ ]  | [ ]  | [ ]  | Permanent Seeding | [ ]  | [ ]  | [ ]  |
| Culvert Pipe Checks | [ ]  | [ ]  | [ ]  | Sod | [ ]  | [ ]  | [ ]  |
| Inlet Protection | [ ]  | [ ]  | [ ]  | Grading Practices | [ ]  | [ ]  | [ ]  |
| Turbidity Barrier | [ ]  | [ ]  | [ ]  |  |  |  |  |
| Rock Bags | [ ]  | [ ]  | [ ]  | Operations in Conformance with ECIP? | [ ]  | [ ]  |  |
| Tracking Pads | [ ]  | [ ]  | [ ]  | Other:       | [ ]  | [ ]  | [ ]  |
| Temporary Diversion Channel | [ ]  | [ ]  | [ ]  | Other:       | [ ]  | [ ]  | [ ]  |
| Temporary Settling Trap/Basin | [ ]  | [ ]  | [ ]  | Other:       | [ ]  | [ ]  | [ ]  |
| Dewatering Operation | [ ]  | [ ]  | [ ]  | Other:       | [ ]  | [ ]  | [ ]  |
| Bypass Pumping Operation | [ ]  | [ ]  | [ ]  | Other:       | [ ]  | [ ]  | [ ]  |

**Note: BMPs checked yes must have Sections 4 and 5 completed. ECIP conformance checked no requires explanation.**

**4. Description and Location of Issue**

|  |  |
| --- | --- |
| **Item** | **Description and Location of Issue (attach pictures if necessary)** |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |

**[ ]  See Attached sheet for additional Description and Location issues or Comments**

**Within 24 hours of completing the inspection, the inspector shall provide the project leader with a copy of the inspection report. Also, this completed inspection report must be posted on-site within 24 hours of completing the inspection. Erosion control order form, DT 1074, must be used to document communication requiring contractor corrective actions or mobilizations.**

**Optional Additional Page for Description and Location of Issue**

|  |  |
| --- | --- |
| **Item** | **Description and Location of Issue** |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |
|       |       |