FIELD EVALUATION CHECKLIST
Wisconsin Department of Transportation
DT1246     6/2006     s.86.07(2) Wis. Stats.

	County
[bookmark: Text1]     
	Highway Number(s)
[bookmark: Text2]     
	Permit Number
[bookmark: Text3]     

	Location
[bookmark: Text4]     

	Date Inspected
[bookmark: Text5]     
	Inspected By
[bookmark: Text6]     



	Was the work done according to permit/plan/drawing?
[bookmark: Check3][bookmark: Check4]|_|  Yes       |_|  No

	

	If not, please briefly describe.
[bookmark: Text9]     

	

	Name of contractor performing the work.
[bookmark: Text10]     




	PERFORMANCE RATING

	ITEMS RATED
	N/A

(0)
	Very Bad

(1)
	Bad

(2)
	Average

(3)
	Good

(4)
	Very Good
(5)

	Final grading
	[bookmark: Text11]     
	[bookmark: Text12]     
	[bookmark: Text13]     
	[bookmark: Text14]     
	[bookmark: Text15]     
	[bookmark: Text16]     

	Drainage
	[bookmark: Text17]     
	[bookmark: Text18]     
	[bookmark: Text19]     
	[bookmark: Text20]     
	[bookmark: Text21]     
	[bookmark: Text22]     

	Erosion control methods
	[bookmark: Text23]     
	[bookmark: Text24]     
	[bookmark: Text25]     
	[bookmark: Text26]     
	[bookmark: Text27]     
	[bookmark: Text28]     

	Work site safety
	[bookmark: Text29]     
	[bookmark: Text30]     
	[bookmark: Text31]     
	[bookmark: Text32]     
	[bookmark: Text33]     
	[bookmark: Text34]     

	Work site cleanup
	[bookmark: Text35]     
	[bookmark: Text36]     
	[bookmark: Text37]     
	[bookmark: Text38]     
	[bookmark: Text39]     
	[bookmark: Text40]     

	Restoration of R/W or highway
	[bookmark: Text41]     
	[bookmark: Text42]     
	[bookmark: Text43]     
	[bookmark: Text44]     
	[bookmark: Text45]     
	[bookmark: Text46]     

	Cooperation
	[bookmark: Text47]     
	[bookmark: Text48]     
	[bookmark: Text49]     
	[bookmark: Text50]     
	[bookmark: Text51]     
	[bookmark: Text52]     

	Traffic control
	[bookmark: Text53]     
	[bookmark: Text54]     
	[bookmark: Text55]     
	[bookmark: Text56]     
	[bookmark: Text57]     
	[bookmark: Text58]     

	Total Performance Rating
(Add ratings in each column)
	[bookmark: Text59]     
	[bookmark: Text60]     
	[bookmark: Text61]     
	[bookmark: Text62]     
	[bookmark: Text63]     
	[bookmark: Text64]     



	GRAND TOTAL PERFORMANCE RATING of the above columns
	=
	[bookmark: Text66]     

	
	
	

	AVERAGE PERFORMANCE RATING – Divide the Grand Total by the number of items rated.  (Do not include “Not Applicable” (N/A) ratings)
	=
	[bookmark: Text67]     

	
	
	

	Pictures Taken?
	[bookmark: Check1]|_|  Yes 
	[bookmark: Check2]|_|  No



Other Comments





PERFORMANCE RATINGS

	5 -
	VERY GOOD
	Exceptional work effort and product, performance consistently exceeds requirements.

	
	
	

	4 -
	GOOD
	Performance is above average.  All requirements of the job are met and often exceeded.

	
	
	

	3 -
	AVERAGE
	Performance is average.  Some work may need improvement.

	
	
	

	2 -
	BAD
	Performance is below average.  Indicates significant need for improvement.  Some aspect of the work needs to be redone or will cause future problems.

	
	
	

	1 -
	VERY BAD
	Performance is poor and unacceptable.  The work should be redone and the company should be notified.




ITEM DEFINITIONS

Final grading - All excavated slopes or areas should be covered with 4 inches of topsoil.  The earth grade shall be trimmed and finished to merge with adjacent terrain and conformity with existing roadway and right-of-way cross sections and drainage patterns.

Drainage - The finish grading of the project should not impede the natural or pre-existing flow of surface water or stream in any unreasonable manner so as to cause accumulation of water or water soaking, flooding or water soaking within the right of way or adjacent private property.

Erosion Control - The work shall be done in accordance with Trans 401, Wis. Adm. Code.  The contractor is responsible for the control of water pollution, erosion and situation at the worksite.

Work Site Cleanup - Upon completion of work, the contractor shall remove from the right-of-way and affected adjacent property all surplus and discarded materials, rubbish, and equipment and leave the work site area in a neat and presentable condition.

Restoration of R/W and Highway - Requires contractor to restore right-of-way and highway facilities to pre-existing conditions.

Cooperation - Consider the following:  Was the contractor responsive to requests or suggestions?  Did the contractor react well to criticism?  Was it difficult to work with the contractor?  Was the contractor courteous and helpful in dealing with you and the public?

Traffic Control - Traffic during all work shall conform to the current “Wisconsin Manual on Uniform Traffic Control Devices”.  This assures safety to the traveling public and people working on the job.
