SIGN STRUCTURE INSPECTION REPORT
Wisconsin Department of Transportation
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	District
[bookmark: Text1]     
	County
[bookmark: Text2]     
	Highway
[bookmark: Text3]     
	Structure Number
[bookmark: Text4]     

	Location
[bookmark: Text5]     
	Station
[bookmark: Text6]     

	Bridge Type
	
	Approximate Length
[bookmark: Text8]     

	[bookmark: Check5]|_| Aluminum
	[bookmark: Check6]|_| Steel
	



	Item
	Check When Attention May Be Req’d
	Comment
(Attention or Action Required)

	Superstructure
	[bookmark: Check1]|_|
	[bookmark: Text12]     

	Truss
	[bookmark: Check2]|_|
	[bookmark: Text13]     

	Upper-Lower Chords
	[bookmark: Check3]|_|
	[bookmark: Text14]     

	Cracks in Pipe
	[bookmark: Check4]|_|
	[bookmark: Text15]     

	Cracks in Welds
	|_|
	[bookmark: Text16]     

	Flange Couplings
	|_|
	[bookmark: Text17]     

	Diagonals and Struts
	|_|
	[bookmark: Text18]     

	Cracks in Pipe
	|_|
	[bookmark: Text19]     

	Cracks in Welds
	|_|
	[bookmark: Text20]     

	Unusual Vibration Detected
	|_|
	[bookmark: Text21]     

	Corroding Hardware – Fasteners (metal type)
	|_|
	[bookmark: Text22]     

	Loose Hardware – Fasteners
	|_|
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	Walkway and Railings
	|_|
	[bookmark: Text24]     

	Paint (peeling, rust, primer showing)
	|_|
	[bookmark: Text25]     

	Towers
	|_|
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	Cracks in Main Members (welds, pipe)
	|_|
	[bookmark: Text27]     

	Cracks in Struts or Diagonals
	|_|
	[bookmark: Text28]     

	Handhole and Cover
	|_|
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	Paint (peeling, rust, primer showing)
	|_|
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	Substructure
	|_|
	[bookmark: Text31]     

	Footings
	|_|
	[bookmark: Text32]     

	Concrete Cracks
	|_|
	[bookmark: Text33]     

	Differential Settlement
	|_|
	[bookmark: Text34]     

	Grout Cracking
	|_|
	[bookmark: Text35]     

	Base Castings and Anchor Bolts (metal type)
	|_|
	[bookmark: Text36]     

	Sign Lighting
	|_|
	[bookmark: Text37]     

	Apparent Defects
	|_|
	[bookmark: Text38]     

	Signs
	|_|
	[bookmark: Text39]     

	Unsatisfactory Appearance (specify)
	|_|
	[bookmark: Text40]     

	Damaged or Deteriorated
	|_|
	[bookmark: Text41]     

	Damaged or Loose Attachment Devices
	|_|
	[bookmark: Text42]     

	Bridge Number
	|_|
	[bookmark: Text43]     

	Missing, Peeling or Faded
	|_|
	[bookmark: Text44]     

	Crash Protection
	|_|
	[bookmark: Text45]     

	Type/Condition (guardrail, attenuator, barrier)
	|_|
	[bookmark: Text46]     

	Distance from Edge of Driving Lane to CL Support
	|_|
	[bookmark: Text47]     


Remarks


Page 1 of 2



	Date
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	Inspected By
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Instructions
Sign Structure Inspection Report
DT2018

* - Indicates that a particular item will most often be pre-printed on the Inspection Report, if applicable.  However, the inspector should verify the item’s accuracy, and update the information if it is not correct.

· District* - The district where the inspection was performed.

· County* - The county in which the sign bridge is located.  If the structure is located on a county line, then the lower number county is entered here.

· Highway* - The highway over which the sign bridge spans.

· Structure Number* - The number assigned by the governing WisDOT District Office that uniquely identifies a structure for the inventory database.  Refer to Part 1 Section 5.2 for the standard format.
	Note:  If a unique number has not been assigned by WisDOT, use this line to identify the component by specific name, location, or by Structure No. of the adjacent structure.

· Location* -  A distance and a direction to the structure from another landmark commonly found on a state roadmap, usually another roadway.

· Station* - The numerical station location of the sign bridge.

· Bridge Type* - Note the structure material in this field.  Usually, these structures are either aluminum or steel.

· Approx. Length* - Enter the approximate length of the sign bridge.


Superstructure - Check each defect that applies for the truss, diagonals, and struts, and make pertinent comments as to the nature of the defect.

Substructure - Check each defect that applies for the footings, and make pertinent comments as to the nature of the defect.

Sign Lighting - Check any apparent defects for the lighting potion of the sign bridge, and make any pertinent comments as to the nature of the defect.

Signs - Check any appropriate defects that relate to the condition of the signs, and make any pertinent comments as to the nature of the defect.

Bridge Number - Check the appropriate defect that relates to the condition of the sign structure identification plate, and make any pertinent comments as to the nature of the defect.

Crash Protection - Check the appropriate defect that relates to the condition of the crash protection, and make any pertinent comments regarding the nature of the defect. 

Date - The date the current inspection is being performed.

Inspected By - The inspector performing the current inspection.

